en	Vertebral train unit A
nl	Vertebrale trein unit A

en	Vertebral train unit B
nl	Vertebrale trein unit B

en	Vertebral train unit C
nl	Vertebrale trein unit C

en	Vertebral Train Goicoechea
nl	Vertebrale Trein Goicoechea

en	Vertebral train depot
nl	Vertebrale treindepot

en	Vertebral train station
nl	Vertebrale treinstation

en	Vertebral train tunnel
nl	Vertebrale treintunnel

en	Vertebral train beams
nl	Vertebrale treinbalken

en	Vertebral train pre-signal
nl	Vertebrale trein voorsein

en	Vertebral train signal
nl	Vertebrale trein sein

en	Vertebral train system
nl	Vertebrale treinsysteem

en	The vertebrate train of Las Palmas de Gran Canaria this vehicle required, by its own design, a track totally incompatible with the existing railway network, based on long concrete beams on which the composition supported by independent treads located on the sides of the vehicle and not in its lower part, as is usual in conventional trains or cars. According to its inventor, in this way it was achieved that the train was non-derailing, by placing the center of gravity in the same plane as the additional guide wheels and, therefore, the tipping torque was zero.
nl	De vertebrale trein van Las Palmas de Gran Canaria vereiste, omwille van het ontwerp, een spoor dat volledig incompatibel was met het bestaande spoornetwerk. Dit ontwerp was gebaseerd op lange betonnen balken waarop de trein hing, ondersteund door wielen aan de zijkant van het voertuig in plaats van de onderzijde zoals meer conventionele treinen of auto's. Volgens de uitvinder kon de trein op deze manier niet ontsporen omdat het zwaartepunt zich op hetzelfde vlak bevond als de geleidingswielen en het kantelmoment op deze manier gelijk was aan nul.