en	Vertebral train unit B

en	Vertebral train unit C

en	Vertebral Train Goicoechea

en	Vertebral train depot

en	Vertebral train station

en	Vertebral train tunnel

en	Vertebral train beams

en	Vertebral train pre-signal

en	Vertebral train signal

en	Vertebral train system

en	The vertebrate train of Las Palmas de Gran Canaria this vehicle required, by its own design, a track totally incompatible with the existing railway network, based on long concrete beams on which the composition supported by independent treads located on the sides of the vehicle and not in its lower part, as is usual in conventional trains or cars. According to its inventor, in this way it was achieved that the train was non-derailing, by placing the center of gravity in the same plane as the additional guide wheels and, therefore, the tipping torque was zero.